**THỰC TRẠNG ĐIỀU KIỆN LAO ĐỘNG CỦA CÔNG NHÂN**

**TẠI CÔNG TY XI MĂNG VICEM HẢI PHÒNG NĂM 2013**

**Đỗ Mạnh Cường\***

**TÓM TẮT[[1]](#footnote-1)**

Năm 20013, tiến hành khảo sát điều kiện lao động của công nhân làm việc tại công ty Xi Măng Vicem Hải Phòng, kết quả cho thấy:

**Môi trường lao động**: Nhiệt độ đạt Tiêu chuẩn cho phép (TCCP) chung tại các điểm đo là 61,43%, trong đó tại xưởng nghiền - đóng bao đạt 20%, xưởng nguyên liệu 72,5%, xưởng điện 100%. Tỉ lệ đạt TCCP mẫu ồn chung tại các điểm đo là 57,14%, ánh sáng là 94,2%. Trong đó ở xưởng điện đạt 90%, xưởng nghiền - đóng bao 65%, xưởng nguyên liệu 35%. Ánh sáng đạt TCCP ở xưởng nghiền - đóng bao 100%, xưởng nguyên liệu 92,5% và xưởng điện 90%. Đạt TCCP mẫu bụi toàn phần chung là 76%, bụi hô hấp 100%.Trong đó xưởng điện đạt 100%, xưởng nguyên liệu 79,2% và xưởng nghiền - đóng bao 58,8%.

**Điều kiện lao động**: Tỷ lệ công nhân cảm thấy có bụi 91,6%, có ồn 53,9%, có nóng 27,2%. Công nhân được trang bị bảo hộ lao động 100%, tỉ lệ sử dụng bảo hộ lao động (BHLĐ) từ 99,4 - 100%. Công nhân làm việc trong môi trường có các hệ thống đảm bảo điều kiện làm việc từ 82,2% - 98,4%,có hệ thống hút hơi khí độc 50,8%.

**SUMMARY**

**WORKING CONDITIONS OF**

**WORKERS AT VICEM HAI PHONG**

**CEMENT FACTORY IN 2013**

A research on working conditions of workers at Vicem Hai Phong cement factory in 2013 showed that:

**Working Environment**: The average temperature within the acceptable standard at the observation points is 61.43%, of which the temperature at the grinding and packaging department is 20%, at raw materials department is 72.5% and at the electricity department is 100%. The average noise level within the acceptable standard at the observation points is 57.14% and the average light level is 94.2%. Of which the noise level at the electricicty department is 90%, at the grinding and packaging department is 65%, at the raw material department is 35%. The light level at the grinding and packaging department is 100%, at the raw material department is 92.5% and at the electricity department is 90%. The average total dust level within the acceptable standard is 76% and the average respiratory dust level within the acceptable level is 100%. Of which, the dust level at the electricity department is 100%, at the raw material department is 79.2% and at the grinding and packaging department is 58.8%.

**Working conditions:** 91.6% of workers feel dusty, 53.9% feel noisy and 27.2% feel hot. 100% of workers are equipped with protective clothes; the percentage of workers using protective clothes is 99.4% to 100%. 82.2% - 98.4% of workers working in well facilitated environment and 50.8% of the departments are facilitated with poisonous gas exhaustion system.

1. [↑](#footnote-ref-1)